**LOT 5: Supply of food processing related Equipment and Materials to be supplied to Musanze and Rubavu District**

*Bidders are expected to examine carefully and comply with all instructions and specifications.*

**Date: \_\_\_\_\_\_/\_\_\_\_\_\_/\_\_\_\_\_\_\_\_\_**

**Bidder Information**

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
| Bidder’s Legal Name |  |  |
|  |
| TIN Number |  |  |
|  |  |  |
| Country/ies of Registration/Operation |  |  |
|

|  |
| --- |
|  |

Bidder’s Authorized Representative |
|  |  |  |  |  |
| Title |  |  Telephone |  |  |
|  |
| Email |  |  |
|  |

**Descriptions and Specifications of food processing related Equipment and Materials to be supplied to Musanze and Rubavu District**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Item No** | **Item** | **Item Specification** | **Units** | **Quantity** | **Unit Price (Frw)** | **Total Price (Frw)** |
| 1 | Meat cutter | Size (48\*380mm), Model (250), Power (1.5KWH), Voltage (220V), Weight (42KG) | PC | 1 |  |  |
| 2 | Meat mincer | Size (medium), model (SR-D100), power (ELECTRIC), voltage (220V) and weight (45Kg)  | PC | 1 |  |  |
| 3 | Meat refrigerator | Meat Hanging, Meat display refrigerator Aged Fridge Cabinet Refrigeration Meat Hanging Display Storage Room | PC | 1 |  |  |
| 4 | Milk Cooling Tank | Origin: Turkey (Europe), Capacity:500L, Direct expansion open milk cooler, Vertical cylindrical tank with opening lid, Manufactured in AISI 304 stainless-steel and compliant with the most stringent food-processing requirements, Compliant with standards ISO 5708 and EN 13732, DN50 Discharge Valve, Material Stainless Steel AISI 304 R404 or R410 Coolant Freon gas, One Agitator Motor  | PC | 1 |  |  |
| 5 | Pasteurizer machine | Origin: Turkey, Capacity:500L, 380V,45Kw, Vertical cylindrical tank with opening lid, Manufactured in AISI 304 stainless steel and compliant with the most stringent food-processing requirements, Material Stainless Steel AISI 304 and One Agitator Motor | PC | 1 |  |  |
| 5 | Milking Cans | Capacity: 50 Litres, Usage/Application: For milk collection, Weight: 8.6 kg, Weight: 8.6 kg, Surface Treatment: Polished, Material: Stainless Steel, Country of Origin: Turkey | PCs | 10 |  |  |

**NOTE:**

1. Kilimo Trust Rwanda, in a fair and transparent manner, will select companies that fulfill all requirements.
2. Interested bidders must visit the site any time before the deadline period **31st March 2025**.
3. For items that need to be installed or assembled, the bidder should include installation and assembling cost in the bid.